# ROMEO

A staggered 40% that can be assembled with only through hole components, including usb type-c, and can also be completely covered with most GMK base kits

* Keyboard Maintainer: [coseyfannitutti](https://github.com/coseyfannitutti)
* Hardware Supported: ROMEO, ATmega328P
* Hardware Availability: [cftkb.com](http://www.cftkb.com), [GitHub](https://github.com/coseyfannitutti/romeo)

Make example for this keyboard (after setting up your build environment):

    make coseyfannitutti/romeo:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
