# The default ISO keymap for baguette

Typical ISO keymap. Please note:
- Left key from split backspace is connected to 2u key.
- Left key from split left Shift is connected to 2u key.
- Right key from split right Shift is connected to 2u key.
- Backlight control is on the Z, X and C keys of the FN layer.
- Reset key combination is FN + ].
- Holding ESC and Space while plugging in the USB erases the EEPROM.

