The default keymap for ISO HS60 V2. VIA support enabled.
========================================================

![Layout image](https://imgur.com/6go4vQV.png)

Default layer is normal ISO and Fn layer is used for RGB functions, Volume control and arrow cluster