# The Six Shooter

A PCB for the CM Storm switch tester utilizing a Teensy 2.0 designed by Bpiphany. Because the PCB was designed with individual pins for each LED, there are custom keycodes (`SS_LON` and `SS_LOFF`) for turning on and off the backlight LEDs.

Keyboard Maintainer: QMK Community  
Hardware Supported: Six Shooter PCB, Teensy 2.0  
Hardware Availability: [GeekHack.org](https://geekhack.org/index.php?topic=70033.0)

Make example for this keyboard (after setting up your build environment):

    make bpiphany/sixshooter:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
