# Prime_L V1

![Prime_L V1](https://i.imgur.com/jUWhjOD.jpg)

A compact layout with the footprint of your typical 65% board, featuring a left mini-numpad. Pre-drilled and counter sunk holes for use with optional feet for a slight tilt. Switches are oriented so that back light LEDs are on the top of the switch.

* Keyboard Maintainer: [MxBlue](https://github.com/MxBlu)
* Hardware Supported: Prime_L V1 PCBs, ATmega32u4  
* Hardware Availability: V1 PCB no longer produced

Make example for this keyboard (after setting up your build environment):

    make primekb/prime_l/v1:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
