# FaceW

A 60% no frills keyboard.

The FaceW is a special run of the WKL B.Face sourced from Sprit that doesn't have underglow RGB LEDs but does have in switch LEDs. Also unlike the B.Face, it is based on ps2avru instead of ps2avrGB. It is designed and manufactured in Korea. 

* Keyboard Maintainer: [MechMerlin](www.github.com/mechmerlin)
* Hardware Supported: FaceW Sprit Edition PCB
* Hardware Availability: <https://mechanicalkeyboards.com/shop/index.php?l=product_detail&p=1352>

Make example for this keyboard (after setting up your build environment):

    make facew:default

Flashing example for this keyboard ([after setting up the bootloadHID flashing environment](https://docs.qmk.fm/#/flashing_bootloadhid))

    make facew:default:flash

**Reset Key**: Hold down the key located at *K01*, commonly programmed as *q* while plugging in the keyboard.

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
