# Red Scarf II+ Ver.B (RS78)

A 65% keyboard with two function columns on the left.

Keyboard Maintainer: [Maartenwut](https://github.com/Maartenwut)  
Hardware Supported: Ver.B (RS78), Ver.C (RS68)  
Hardware Availability: [Drop](https://drop.com/buy/red-scarf-ii-ver-b-custom-mechanical-keyboard-kit)

Please note that when QMK firmware is flashed, the remote will cease to control the underglow LEDs. 

## Flashing

The flashing is sub-optimal. 

Flashing the Red Scarf involves using Google Chrome, downloading an extension, and then flashing. For more detailed instructions please refer to [kairyu.gitbooks.io](https://kairyu.gitbooks.io/red-scarf-ii-plus-user-guide-how-to-custom-layout/content/online_reflash.html)

---

Make example for this keyboard (after setting up your build environment):

    make redscarf_iiplus/verb:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
