# HID Liberation Device

DIY daughterboard for Filco Majestouch TKL developed by Geekhack and Deskthority communities. The PCB was engineered by bpiphany.

## Wiki on Deskthority.net
- [Instructions](http://deskthority.net/wiki/HID_Liberation_Device_-_Instructions)
- [Assembly Instructions](http://deskthority.net/wiki/HID_Liberation_Device_-_DIY_Instructions)

* Keyboard Maintainer: [The QMK Community](https://github.com/qmk)
* Hardware Supported: HID Liberation Device (ATmega32U4)
* Hardware Availability: Discontinued

Make example for this keyboard (after setting up your build environment):

    make hid_liber:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
