# P18 

![render](https://i.imgur.com/CPtGiSL.png)

A 18-key DIY Hotswap Macropad that accepts both Pro Micro and Adafruit Feather 32u4 Bluefruit LE.

* Keyboard Maintainer: [pabile](https://github.com/pabile)
* Hardware Supported: Pabile P18 PCB with Pro Micro or Adafruit Feather 32u4 Bluefruit LE
* Hardware Availability: [Info at pabileonline.blogspot.com](https://pabileonline.blogspot.com/search/label/pabile18)

Make example for this keyboard (after setting up your build environment):

    make pabile/p18:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
