# JC65

![JC65 with 32u4](https://i.imgur.com/I4hCyBI.jpg)
![JC65 with 32a](https://i.imgur.com/9cJ9UbX.jpg)

The JC65 is the PCB for the Rama M65-A sold through [keyclack.com](https://keyclack.com/). There are two revisions available, a native QMK powered PCB (v32u4) and a PS2AVRGB PCB (v32a), both are available on keyclack. 

QMK is supported for both variants. 

Make example native QMK version (after setting up your build environment):

    make jc65/v32u4:default

Make example ps2avrGB version (after setting up your build environment):

    make jc65/v32a:default
