# EVE Meteor

60% PCB with Function Row

* Keyboard Maintainer: [MechMerlin](https://github.com/mechmerlin)
* Hardware Supported: EVE Meteor
* Hardware Availability: [zFrontier](https://en.zfrontier.com/products/eve-meteor)

Make example for this keyboard (after setting up your build environment):

    make eve/meteor:default

Flashing example for this keyboard ([after setting up the bootloadHID flashing environment](https://docs.qmk.fm/#/flashing_bootloadhid))

    make eve/meteor:default:flash

**Reset Key:** Short the two holes labeled `FW_JP` underneath the PCB, beside the Tab key while plugging in the keyboard. 

Do not confuse this with the LED holes of the switch in the `Tab` position. `FW_JP` is not reachable from the top as the plate blocks access to it. 

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
