# otaku_split

![otaku_split](https://booth.pximg.net/c/620x620/4394ec37-d0ff-4c92-8f78-5c08d0566da6/i/1398595/511647ef-43e4-4f50-b56d-a0166c090fae_base_resized.jpg)
![otaku_split_bottom](https://booth.pximg.net/c/620x620/4394ec37-d0ff-4c92-8f78-5c08d0566da6/i/1398595/cc9eb113-46a9-42fa-aaed-c4007efbe45e_base_resized.jpg)


This is JP layout based split keyboards.



Keyboard Maintainer: [takashiski](https://github.com/takashiski)  
Hardware Supported: promicro(atmega32u4) on Otaku Split rev.1 PCB  
Hardware Availability: https://skyhigh-works.booth.pm/items/1398595

Make example for this keyboard (after setting up your build environment):

    make otaku_split/rev1:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
