The default keymap for ANSI HS60
================================

![Layout image](https://imgur.com/CSyPw0J.png)

Default layer is normal ANSI and Fn layer is used for RGB functions, Volume control and arrow cluster