# Kira 80/TKL

![kira80](https://i.imgur.com/QnGKnaml.jpg)
![kira80pcb](https://i.imgur.com/wrEZhg5l.jpg)

Custom TKL keyboard designed and made by Thesiscamper and EVE

* Keyboard Maintainer: [elmo-space](https://github.com/elmo-space)
* Hardware Supported: Kira 80 PCB made by EVE
* Hardware Availability: limited [Group Buy](https://geekhack.org/index.php?topic=96381.0) finished

Make example for this keyboard (after setting up your build environment):

    make kira80:default

Flashing example for this keyboard ([after setting up the bootloadHID flashing environment](https://docs.qmk.fm/#/flashing_bootloadhid))

    make kira80:default:flash

**Reset Key:** Hold down the key located at `K102`, commonly programmed as 'Pause' while plugging in the keyboard.

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

## Hardware Information

Controller: ATmega32A

### Pinout:

|Pin |Use      | |Pin |Use            |
|----|---------|-|----|---------------|
|`A1`|Column 0 | |`B1`|Row 0          |
|`A2`|Column 1 | |`B2`|Row 1          |
|`A3`|Column 2 | |`B3`|Row 2          |
|`A4`|Column 3 | |`B5`|Row 3          |
|`A5`|Column 4 | |`B6`|Row 4          |
|`A6`|Column 5 | |`B7`|Row 5          |
|`A7`|Column 6 | |`B0`|Row 6          |
|`C7`|Column 7 | |    |               |
|`C6`|Column 8 | |`D1`|Caps Lock LED  |
|`C5`|Column 9 | |`D6`|Scroll Lock LED|
|`C4`|Column 10| |`D4`|Backlight      |
|`C3`|Column 11| |    |               |
|`A0`|Column 12| |`D2`|USB D+         |
|`C2`|Column 13| |`D3`|USB D-         |
|`D7`|Column 14| |    |               |

### Layout matrix:

![matrix](https://i.imgur.com/FqjTNQS.png)
