# Exclusive E8.5 Soldered

Soldered PCB for Exclusive E8.5.  

* Keyboard Maintainer: [MechMerlin](https://github.com/mechmerlin), [rebeccaby](https://github.com/rebeccaby)
* Hardware Supported: E8.5 Soldered, atmega32u4
* Hardware Availability: [Geekhack GB](https://geekhack.org/index.php?topic=103520)

Make example for this keyboard (after setting up your build environment):

    make exclusive/e85/soldered:default

**Reset Key**: The board can be reset by shorting the two holes underneath the PCB, or pressing the reset button on the reverse side. 

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
