# rask's Pearl 40%

## Layout

The firmware offers five layers:

1. Base layer
2. Base with numbers and symbols (Fn1)
3. Base with F-row and arrows (Fn2)
4. Base with media and RGB controls (Fn3)
5. More nav and utils (Fn2+Fn3, aka NavFn)

![rask's Pearl 40% layout](https://i.imgur.com/gKVQapZ.png)

Base for this firmware copied from jetpacktuxedo's QMK firmware.

---

## Compiling and flashing

To compile a HEX follow the Pearl 40% instructions.

Flashing instructions also available at Pearl 40% instructions.
