# stoutgat

![stoutgat](https://i.imgur.com/CfWa5AGl.jpg?1)

An ISO through hole component 65% keyboard with dual encoders. Uses the ATMega32A.
Inspired by the cftkb Discipline.

* Keyboard Maintainer: [Thys de Wet](https://github.com/vattern)
* Hardware Supported: Stoutgat PCBs , running ATMega32A
* Hardware Availability: https://github.com/vattern/stoutgat

Make example for this keyboard (after setting up your build environment):

    make stoutgat:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
