# PRKL30

![prkl30](https://camo.githubusercontent.com/9b39ee253a7cdcbfdbe80f7ef36ddd3ad5b17382/68747470733a2f2f692e696d6775722e636f6d2f4e6b67493339492e6a7067)

30% Keyboard with ISO Enter, ortho layout and bluetooth support

* Keyboard Maintainer: [ErkHal](https://github.com/erkhal)
* Hardware Supported: PRKL30 PCB, Pro Micro/Adafruit Feather
* Hardware Availability: [PRKL30 repo](https://github.com/erkhal/prkl30)

Make example for this keyboard with Pro Micro controller (after setting up your build environment):

    make handwired/prkl30/promicro:default

Make example for this keyboard with Feather controller (after setting up your build environment):

    make handwired/prkl30/feather:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
