# Eniigma Keyboards ek65

![ek65](https://i.imgur.com/s6DI5vu.png)

A 65% PCB with symmetrical bottom row layout, JST daughterboard support, designed for use with Eniigma Keyboards products.

* Keyboard Maintainer: [eniigmakeyboards](https://github.com/eniigmakeyboards) and [adamws](https://github.com/adamws)
* Hardware Supported: Vertigo PCB/case
* Hardware Availability: On the [Eniigma Keyboards website](https://eniigmakeyboards.com)

Make example for this keyboard (after setting up your build environment):

    make eniigmakeyboards/ek65:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
