# Mousepad layout for BDN9
##### 2 encoders required
Why use a movable mouse when you can "Etech-a-sketch" style mousepad. 
The left encoder will move the X axis; leaving the right to handle the Y axis

|   |   |   |
|:-:|:-:|:-:|
| Left Click | Middle Click | Right Click |
| Scroll Up | Super ALT↯TAB | Scroll Left |
| Scroll Down | ADJUSTMENT Layer | Scroll Right|

|   |   |   |
|:-:|:-:|:-:|
| RESET | Mouse ACL0 | Mouse ACL1 |
| VOL UP | Mouse ACL2 | Brightness UP |
| VOL Down | Adjustment Layer OFF | Brightness Down |
