# bm16a

![bm16a](https://ae01.alicdn.com/kf/HTB1RRRQaZfrK1RjSszcq6xGGFXaY.jpg)

A 16 key macropad, with USB C, RGB underglow and backlight.

Keyboard Maintainer: QMK Community  
Hardware Supported: The PCBs, controllers supported  
Hardware Availability: [KPrepublic](https://kprepublic.com/products/bm16a-16-keys-custom-mechanical-keyboard-pcb-plate-programmed-numpad-layouts-qmk-firmware-with-rgb-bottom-underglow-alps-mx); [AliExpress](https://www.aliexpress.com/store/product/bm16a-16-keys-Custom-Mechanical-Keyboard-PCB-plate-programmed-numpad-layouts-qmk-firmware-with-rgb-bottom/3034003_32970629907.html)

Make example for this keyboard (after setting up your build environment):

    make bm16a:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
