# Mechmini V1

A 40% ortholinear/staggered keyboard, that was originally bootmapper and can be ported to QMK following this readme.  This version is no longer in production [More info on MECHKEYS](https://mechkeys.ca).

* Keyboard Maintainer: QMK Community
* Hardware Supported: Mechmini 1 PCB
* Hardware Availability: Version 1 (Bootmapper) no longer in production [MECHKEYS](https://mechkeys.ca)

Make example for this keyboard (after setting up your build environment):

    make mechmini/v1:default

Flashing example for this keyboard ([after setting up the bootloadHID flashing environment](https://docs.qmk.fm/#/flashing_bootloadhid))

    make mechmini/v1:default:flash

**Reset Key**: Hold down the key commonly programmed as *L_Ctrl* while plugging in the keyboard.

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
