# yanfali's keymap for KBDFans DZ60 PCB

## 4 Layers

### Layer 0

![layer 0](https://imgur.com/gELh7Se.png)
Conventional ANSI layout. Except:

 - Backspace has been replaced with 2 keys
   - PGUP
   - PGDN
 - 2.25U Left shift is now 1.25U with 1U key LT(layer 3, KC_Z)
 - Bottom right shift is 1.75U. Has arrow cluster. Tap right shift for / and dedicated / key is to far right.
 - Bottom row, split space bar
   - 2.75U (Space)
   - 1.25U (mouse key + WASD) with LT(4, KC_SPC)
   - 2.25U (backspace)
   - 1U MO(layer 2)
   - 1U LT(layer 1, SHIFT+LGUI+R)
   - arrows.

### Layer 1

![layer 1](https://imgur.com/X7iKNxQ.png)
RGB underglow and backlight controls, Reset

### Layer 2

![layer 2](https://imgur.com/bOiQI69.png)
F1-F12, PGUP -> HOME, PGDN -> END

### Layer 3

Unused at this time but tied to 3 FN key to right of 1.25U left shift.

### Layer 4

 * WASD - Mouse controls
 * Q - Btn 1
 * E - Btn 2

