# hnah108

![hnah108](https://i.imgur.com/rV0lM8M.jpg)  

A Full size keyboard pcb with rotary encoder. Used ws2811 IC as a indicator LED driver 

Keyboard Maintainer: [HnahKB](https://github.com/vuhopkep)  
Hardware Supported: Hnah108 v1  

Make example for this keyboard (after setting up your build environment):

    make handwired/hnah108:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
