# dumbpad

![dumbpad](https://i.imgur.com/sS3fq1Z.jpg)

A 4x4 macro/numpad with rotary encoder.

Keyboard Maintainer: [imchipwood](https://github.com/imchipwood)

PCB repository: https://github.com/imchipwood/dumbpad

Make example for this keyboard (after setting up your build environment):

    make dumbpad:default

Program with:

    make dumbpad:default:avrdude

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
