# neiso

![neiso](https://i.imgur.com/8uj89kN.jpg)

A ProMicro/Teensy 2.0/Elite C controlled 5 key macropad using 4 ISO enter keys. Initially based on the I-S-hOle macropad.

Keyboard Maintainer: jrfhoutx  
Keyboard Designer: [jrfhoutx](https://github.com/jrfhoutx)  
Hardware Supported: N-E-ISO PCB; ProMicro, Teensy 2.0, Elite C, Proton C  
Hardware Availability: Space City Keyboards

Make example for this keyboard (after setting up your build environment):

    make sck/neiso:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
