# Mars 8.0

TKL Keyboard with in switch backlight and RGB Underglow. 

* Keyboard Maintainer: [MechMerlin](https://github.com/mechmerlin)
* Hardware Supported: Mars 8.0 PCB
* Hardware Availability: [Geekhack Group Buy](https://geekhack.org/index.php?topic=93723.0)

Make example for this keyboard (after setting up your build environment):

    make ft/mars80:default

Flashing example for this keyboard ([after setting up the bootloadHID flashing environment](https://docs.qmk.fm/#/flashing_bootloadhid))

    make ft/mars80:default:flash

**Reset Key:** Hold down the key located at `K00`, commonly programmed as `Pause/Break` while plugging in the keyboard.

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
