# hnah40

![Hnah40](https://i.imgur.com/nXVmcyc.jpg)

A custom 40% keyboard PCB, insprired by Plaid keyboard from hsgw


Keyboard Maintainer: [vuhopkep](https://github.com/vuhopkep)  
Hardware Availability: https://github.com/vuhopkep/PCB/tree/master/Hnah40-Atmega328p

Make example for this keyboard (after setting up your build environment):

    make handwired/hnah40:default

Flashing example for this keyboard:

    make handwired/hnah40:default:flash

## Bootloader 
use usbasploader from hsgw.
https://github.com/hsgw/USBaspLoader/tree/plaid


See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
