The default keymap for HHKB HS60 V2. VIA support disabled.
==========================================================

![Layout image](https://imgur.com/usbrQWL.png)

Default layer is normal HHKB with 7U space. Fn layer is used for RGB functions, Volume control and arrow cluster