# dactyl_left

![dactyl_left](https://i.imgur.com/PYL3Ca2.png)

A custom build of an ergodox dactyl using a Teensy. Pins are custom.

Keyboard Maintainer: [RedForty](https://github.com/RedForty)  
Hardware Supported: Left side of the dactyl only  
Hardware Availability: Custom job

Make example for this keyboard (after setting up your build environment):

    make handwired/dactyl_left:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
