# THE30

![the30](https://i.loli.net/2019/11/06/KTn3dNjreigovRz.jpg)

A 30% custom keyboard designed and produced by [LazyDesigners](http://lazydesigners.cn).

* Keyboard Maintainer: [Erovia](https://github.com/Erovia)
* Hardware Supported: THE30
* Hardware Availability: Check for GBs on [Geekhack](https://geekhack.org) and on [LazyDesigner's homepage.](http://lazydesigners.cn)

Make example for this keyboard (after setting up your build environment):

    make lazydesigners/the30:default

Flashing example for this keyboard ([using the command line](https://docs.qmk.fm/#/newbs_flashing?id=flash-your-keyboard-from-the-command-line)):

    make lazydesigners/the30:default:flash

To enter the bootloader, either press the RESET button on the PCB or the RESET button if the current keymap has one.

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
