# Prime_L V2

![Prime_L V2](https://i.imgur.com/P3P6GUu.jpg)

A compact layout with the footprint of your typical 65% board, featuring a left mini-numpad.

* Keyboard Maintainer: [HoltenC](https://github.com/HoltenC)
* Hardware Supported: Prime_L V2 PCBs, ATmega32u4
* Hardware Availability: [Store Link](https://www.primekb.com)

Make example for this keyboard (after setting up your build environment):

    make primekb/prime_l/v2:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
