# chidori

![Chidori](https://i.imgur.com/QvpLiOvl.jpg)

Yet another split keyboard made with only through-hole components.

* Keyboard Maintainer: [ka2hiro](https://github.com/ka2hiro) [@ka2hiro](https://twitter.com/ka2hiro)
* Hardware Supported: Chidori PCB, ATMEGA328P
* Hardware Availability: [@kagizaraya](https://twitter.com/kagizaraya)

Make example for this keyboard (after setting up your build environment):

    make chidori:default:usbasp

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
