# S7 Elephant

![S7 Elephant](https://i.imgur.com/CaHxKBJ.jpg)

A high-end 70% custom keyboard designed and produced by [jacky](https://geekhack.org/index.php?action=profile;u=63864) from Geekhack.

**Firmware files are SPECIFIC to each revision. Firmware files from rev1 will not work on rev2 and vice versa.** Please use the `.hex` appropriate for your board.

* Keyboard Maintainer: QMK Community
* Hardware Supported: S7 Elephant rev1, rev2
* Hardware Availability: [The GB has had 2 rounds with little chance to run again.](https://geekhack.org/index.php?topic=96434.0)

Make example for this keyboard (after setting up your build environment):

    make s7_elephant/rev1:default # 2018 run
    make s7_elephant/rev2:default # 2019 run

To enter the bootloader, either short the pins on the PCB or the RESET button on the FN layer.

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
