# Gergo

![ErgoTaco](https://i.redd.it/dbcu5i21m3i21.jpg)

It's a Taco with a side of HASL. A 12 key fiesta of a board.

Keyboard Maintainer: [Jeremy Bernhardt](https://github.com/germ)  
Hardware Supported: ErgoTaco  
Hardware Availability: [gboards.ca](http://gboards.ca)  

## Firmware building
Clone the QMK Repo and install dfu-programmer, flash with:

    make ergotaco:default:dfu

And reset your keyboard!

To just test if your build system is sane, try compiling the default keymap using:
   
    make ergotaco:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

## Have an idea? [Reach out to me!](mailto:bernhardtjeremy@gmail.com)
