# Barleycorn

![Barleycorn](https://i.imgur.com/vi3L1HYl.png)

An f-row less compact 1800 kit with only through hole components.

* Keyboard Maintainer: [Yiancar](http://yiancar-designs.com/) and on [GitHub](https://github.com/yiancar)
* Hardware Supported: ATMEGA328p with vusb [PCB](https://github.com/yiancar/gingham_pcb)
* Hardware Availability: https://mykeyboard.eu/, https://novelkeys.xyz

Make example for this keyboard (after setting up your build environment):

    make barleycorn:default

Flashing example for this keyboard:

    make barleycorn:default:flash

Bootloader:
use usbasploader from HSGW's repository.
https://github.com/hsgw/USBaspLoader/tree/plaid

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
