# KBDPad MKI

Custom numpad. The MKI shares the same ATmega32A and matrix layout as the newer V2 PCB (not to be confused with the MKII, which uses an ATmega32U2!).

* Keyboard Maintainer: [MechMerlin](https://github.com/mechmerlin)
* Hardware Supported: KBDPad MKI, KBDPad V2
* Hardware Availability: [KBDfans](https://kbdfans.com/collections/20/products/kbdfans-kbdpad-pcb-v2)

Make example for this keyboard (after setting up your build environment):

    make kbdfans/kbdpad/mk1:default

Flashing example for this keyboard ([after setting up the bootloadHID flashing environment](https://docs.qmk.fm/#/flashing_bootloadhid))

    make kbdfans/kbdpad/mk1:default:flash

**Reset Key:** Hold down the key located at `K00`, commonly programmed as `0` while plugging in the keyboard.

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
