# Sneakbox Alice Clone PCB

![Sneakbox Alice Clone PCB](https://i.imgur.com/pMZNqLXl.jpg)

An Alice-compatible PCB with hotswap, and pushbutton rotary encoder socket placed at the top left key position. Firmware covers all USB-connector variants of the Sneakbox Alice Clone PCB (Top USB-C, Bottom USB-C)

* Keyboard Maintainer: [mujimanic](https://github.com/mujimanic)
* Hardware Supported: Any Alice-layout case.
* Hardware Availability: [sneakbox.design](https://sneakbox.design/products/sneakbox-alice-hotswap-pcbs)

Make example for this keyboard (after setting up your build environment):

    make sneakbox/aliceclone:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
