# Duck Lightsaver V3

![Lightsaver V3](https://i.imgur.com/Vz23Dkel.jpg)

Non official firmware for custom Korean keyboard with 96 key layout made by Duck.  
Group buy was run 2017 May via [geekhack](https://geekhack.org/index.php?topic=89546.0) and limited to 100 units.

Keyboard Maintainer: [Rasmus Schults](https://github.com/rasmusx)  
Hardware Supported: Lightsaver PCB Ver 3.0, Atmega32u4  
Hardware Availability: [geekhack](https://geekhack.org/index.php?topic=89546.0)

Make example for this keyboard (after setting up your build environment):

    make lightsaver:default

See [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) then the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information.

## Notes
Thanks to Ralf Schmitt for previous implementations in his [TMK fork](https://github.com/xauser/tmk_keyboard/tree/xauser/) and few helping words.
