# Noodle Pad v1 Keypad with Encoder

![NoodlePad TOP](https://static.wixstatic.com/media/59d0ff_052f27ee5ae84266821af7277c51c4ed~mv2.jpg)
![NoodlePad RGB](https://static.wixstatic.com/media/59d0ff_c91f2adc258547a38cc5b480a8d9c510~mv2.jpg)

The Noodle Pad by The Mad Noodle Prototypes is a custom 3x3 mechanical keypad with an encoder knob and full RGB Underglow.

* Keyboard Maintainer: [The Mad Noodle Prototypes](https://github.com/The-Mad-Noodle)
* Hardware Supported: NoodlePad PCB, ATmega32U4
* Hardware Availability: [MadNoodlePrototypes.com](https://www.madnoodleprototypes.com/shop)

Make example for this keyboard (after setting up your build environment):

    make themadnoodle/noodlepad:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. 
Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
