# Speedo

![Speedo](https://raw.githubusercontent.com/pcewing/speedo/master/build_log/images/04-03_23-09-56_00.jpg)

Keyboard Maintainer: [Paul Ewing](https://github.com/pcewing)  
Hardware Supported: Teensy 2.0  
Hardware Availability: You will have to get the plates cut by an online service such as Ponoko. Case files are available in the [Speedo Repository](https://github.com/pcewing/speedo).

Make example for this keyboard (after setting up your build environment):

    make speedo:default

See [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) then the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information.

## Flashing the Firmware
See the QMK docs for handwiring a keyboard; there is a section with instructions on how to flash the *.hex* file to the Teensy 2.0 controller.
