# ASH-XIIX

![ASH-XIIX](https://i.imgur.com/KJk9dDol.jpg)

In mission to fill my Cherry 1800 case. So I continue developing 1800 PCB (ASH-1800) to fit G80-1800 case. It has some update to make ASH-XIIX more user friendly.

* Keyboard Maintainer: [sh_xguitar](https://github.com/sh-xguitar)
* Keyboard Specification: ATmega32u4, 5P TH MINI USB, JST-PH 5P, Larger ISP Header.
* Hardware Availability: Sold in Indonesia only

Make example for this keyboard (after setting up your build environment):

    make ash_xiix:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
