# [RARTPAD](https://github.com/alabahuy/RART/tree/master/RARTPAD)

![rartpad](https://user-images.githubusercontent.com/67696967/86514870-3931bf00-be3f-11ea-8177-29e80add2ce4.jpeg)
5x4 Macropad pcb with double encoder, based on IMKG (Indonesia Mechanical Keyboard Group)

* Keyboard Maintainer: [Alabahuy](https://github.com/alabahuy)
* Hardware Supported: RARTPAD PCB, Promicro, Mini USB, Encoders
* Hardware Availability: Private GB

Make example for this keyboard (after setting up your build environment):

    make rart/rartpad:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
