# Handwired Preonic

A compact 50% (12x5) ortholinear keyboard.

* Keyboard Maintainer: [Daniel Reibl](https://github.com/riblee)
* Hardware Supported: Blackpill F401

Make example for this keyboard (after setting up your build environment):

    make handwired/riblee_f401:default 

Flashing example for this keyboard:

    make handwired/riblee_f401:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).