# TG4x v2.1

40% sandwich keyboard driven by a pro micro. 

For more info please refer to [MythosMann's GitHub](www.github.com/MythosMann/tg4x).  

* Keyboard Maintainer: [MechMerlin](https://github.com/mechmerlin)
* Hardware Supported: TG4x v2.1 PCB
* Hardware Availability: [Geekhack](https://geekhack.org/index.php?topic=99163.0)

If soldering in a RGB underglow strip, please use pin D2, the pin labeled RXI on the pro micro.  

Make example for this keyboard (after setting up your build environment):

    make tg4x:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
