The default keymap for ANSI HS60 V2. VIA support disabled.
==========================================================

![Layout image](https://i.imgur.com/m8t5CfE.png)

Default layer is normal ANSI and Fn layer is used for RGB functions, Volume control and arrow cluster.