# B.fake

A 60% keyboard with RGB. The B.fake pcb is a copy of the B.face PCB sold by [winkeyless](https://winkeyless.kr/). However, the switch matrix is actually the same as the [FaceW](https://github.com/qmk/qmk_firmware/tree/master/keyboards/facew), a ps2avr PCB sold on [mechanicalkeyboards.com](https://mechanicalkeyboards.com/).

* Keyboard Maintainer: QMK Community
* Hardware Supported: B.fake PCB
* Hardware Availability: <https://www.aliexpress.com/store/product/bface-60-RGB-underground-copy-pcb-from-china-gh60-pcb-Customize-keyboard-PCB/2230037_32731084597.html>

Make example for this keyboard (after setting up your build environment):

    make bfake:default

Flashing example for this keyboard ([after setting up the bootloadHID flashing environment](https://docs.qmk.fm/#/flashing_bootloadhid))

    make bfake:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
