# panc60

![panc60](https://imgix.ttcdn.co/i/product/original/0/670893-eca4599c4aad489dbe62609ac2fed86e.jpeg?q=100&auto=format%2Ccompress&w=500)

The panc60 is a 60% PCB with backlight and rgb underglow.   

* Keyboard Maintainer: [MechMerlin](https://github.com/mechmerlin), [Jack Humbert](https://github.com/jackhumbert)
* Hardware Supported: panc60 PCB
* Hardware Availability: [PANC Interactive](https://store.panc.co/product/panc60-60-pcb)

Make example for this keyboard (after setting up your build environment):

    make panc60:default

Flashing example for this keyboard ([after setting up the bootloadHID flashing environment](https://docs.qmk.fm/#/flashing_bootloadhid))

    make panc60:default:flash

**Reset Key**: Hold down the key located at *K40*, commonly programmed as *left control* while plugging in the keyboard.

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
