# mf68

![mf68](https://3.bp.blogspot.com/-0YCA3Hx2Rq0/WD3U3GWhyvI/AAAAAAAB_Uo/RWTeyCPblGcxDrDwT9WL9ck2ZRuR26DgACLcB/s640/IMG_20161129_063741.jpg)
===

Magicforce 68 with [replacement PCB](https://github.com/di0ib/tmk_keyboard/tree/master/keyboard/mf68) designed by [di0ib](https://github.com/di0ib).

* [The original TMK firmware](https://github.com/di0ib/tmk_keyboard/tree/master/keyboard/mf68)

Keyboard Maintainer: QMK Community
Hardware Supported: Pro Micro  
Hardware Availability: [PCB files](https://github.com/di0ib/tmk_keyboard/tree/master/keyboard/mf68/pcb)  

Make example for this keyboard (after setting up your build environment):  

    make 40percentclub/mf68:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
