# YDKB Chili

[Chili PCB](https://i.imgur.com/fKi896a.jpg)

The YDKB Chili is a Cherry G80-3000 replacement PCB utilizing the ATmega32U4 microcontroller.

* Keyboard Maintainer: QMK community
* Hardware Supported: YDKB Chili
* Hardware Availability: [TaoBao](https://item.taobao.com/item.htm?id=565823984744)

Make example for this keyboard (after setting up your build environment):

    make chili:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
